transmission coeff.(%)

960 kev e-/e+, transmission through lead

0

20

40

60

80

100

50 100 150 200 250 300

GEANT4 e-

GEANT4 e+

data e-

ETRAN e-

data e+

ETRAN e+

thickness(mg/cm2)